
TC-C35US 3LRA-4
5MP Fixed Color Maker Bullet Camera
Lite Series
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KEY FEATURES
• Metal housing
• Up to 5MP,3072×1728@30fps
• S+265/H.265/H.264B/H.264M/H.264H
• Color:0.002Lux@(F1.6,AGC ON),B/W:0Lux with IR
• IR range up to 80m
• 1×Built-in Mic
• Support microSD/microSDHC/microSDXC card,up to 512GB
• Support human/vehicle classification
• Operating conditions -35℃~65℃(-31℉~149℉), ≤95%RH
• DC12V±25%,Max. 8W, PoE:IEEE 802.3af,Max. 9W


• IP67
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SPECIFICATIONS
	Camera 
	

	Image Sensor 
	1/2.7"CMOS 

	Min. Illumination 
	Color:0.002Lux@(F1.6,AGC ON),B/W:0Lux with IR 

	Shutter Time 
	1s~1/100000s 

	Day&Night 
	IR-cut filter with auto switch (ICR) 

	Smart IR 
	Yes 

	WDR 
	120dB 

	S/N 
	>39dB 

	Angle Adjustment 
	0~360°(P); 0~90°(T); 0~360°(R) 



	Lens 
	

	Lens Type 
	Fixed focal lens 

	Focal Length 
	4mm 

	Lens Mount 
	M12 

	Aperture Range 
	F1.6 

	Aperture Type 
	Fixed 

	Field of View 
	91°(H); 46.4°(V); 107°(D) 



	DORI Distance 
	Detect:80m 
Observe:31.5m 
Recognize:16m



	Identify:8m 



	Illuminator 
	

	IR LEDs 
	4 

	IR Distance 
	Up to 80m 









	Wavelength 
	850nm 

	White LEDs 
	4 

	Whitelight Distance 
	15m 



	Compression Standard 
	

	Video Compression 
	S+265/H.265/H.264B/H.264M/H.264H 

	Video Bit Rate 
	32k~6Mbps 

	Audio Compression 
	G.711A/G.711U/ADPCM_D 

	Audio Sampling Rate 
	8kHz/32kHz/48kHz 



	Image 
	

	Max. Resolution 
	5MP,3072×1728@30fps 

	Main Stream 
	PAL:25fps(3072×1728, 2688×1520, 2560×1440, 2304×1296, 1920×1080, 1280×720) NTSC:30fps(3072×1728, 2688×1520, 2560×1440, 2304×1296, 1920×1080, 1280×720) 

	Sub Stream 
	PAL:25fps(704×576, 704×288, 640×360, 352×288) NTSC:30fps(704×480, 704×240, 640×360, 352×240) 

	BLC 
	Yes 

	HLC 
	Yes 

	AGC 
	Yes 

	3D DNR 
	Yes 

	White Balance 
	Auto/Semi-Auto/Manual/Sunshine/Nature Light/Warmlight Lamp/Daylight Lamp/ Filament Lamp/Lock White Balance 

	ROI 
	8 rectangular static areas 

	OSD 
	Overlay of additional characters in 1 regions, 1 line, with a maximum of 48 characters or 16 Chinese characters per region; 16*16/32*32/48*48/64*64/96*96; Lattice 

	Privacy Mask 
	4 black static areas 

	Defog 
	Yes 



	Feature 
	

	General Alarm 
	Motion Detection; Mask Alarm 

	Exceptions Alarm 
	Disk Full; Disk R/W Error; IP Address Conflict; Network Disconnection 








	Linkage Method 
	Trigger Recording; Trigger Capture; Notify Surveillance Center 

	Video Analytics 
	Human/Vehicle Classification; Tripwire; Perimeter 

	Rules of Behavior Analyse In 1 Scene 
	2 



	Network 
	

	ANR 
	Yes 

	Protocols 
	RTSP; HTTP; HTTPS; TCP; UDP; UPnP; ICMP; SNMP v1\v2\v3; DHCP; DNS; DDNS; Easy DDNS; NTP; TLS v1.2; QoS; IPv4; SSH; Unicast; Multicast; ARP; FTP 

	System Compatibility 
	P2P(Mutually exclusive with Profile G); ONVIF(Profile S/T/G) ; SDK; CGI; Milestone 

	Remote Connection 
	≤2 

	Client 
	Easy7 VMS 

	Moblie Client 
	EasyLive Plus 

	Web 
	IE10+; Firefox52+; Edge89+; Safari11+; Chrome57+ 



	Interface 
	

	Communication Interface 
	1×RJ-45 (10/100 Base-T) 

	Built-in Mic 
	1×Built-in Mic 

	Reset Button 
	Yes 

	On-board Storage 
	Support microSD/microSDHC/microSDXC card,up to 512GB 

	RTC 
	Yes 



	General 



	Web Client Language 
	20 languages 
Simple Chinese/Traditional Chinese/English/Spanish/Korean/Italian/Turkish/Russian/ Thai/French/Polish/Dutch/Hebrew/Arabic/Vietnamese/German/Ukrainian/Portuguese/



	
	Albanian/Greek 

	Operating Temperature 
	-35℃~65℃(-31℉~149℉) 

	Operating Humidity 
	≤95%RH 

	Storage Temperature 
	-35℃~65℃(-31℉~149℉) 

	Storage Humidity 
	10%~95%RH(non-condensing) 










	Power Supply 
	DC12V±25%,Max. 8W; PoE:IEEE 802.3af,Max. 9W 

	Protection 
	Surge4000V; ESD6000V; IP67 

	Boundary Dimensions 
	239(L)90(W)90(H)mm 

	Package Dimensions 
	280(L)125(W)140(H)mm 

	GrossWeight 
	1.147kg 


DIMENSIONS (Unit: mm) 
[image: ]
Assembly diagram of Junction Box 
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TC-P54BM Spec:V5 A36
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