
TC-H324S 323IA 
PTZ Camera
Pro Series
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KEY FEATURES 
Up to 2MP,1920×1080@30fps 
Color:0.001lux@ (F1.5,AGC ON),B/W:0lux with IR 
S+265/H.265/H.264B/H.264M/H.264H/Motion JPEG 
Optical zoom 23X 
IR range up to 150m 
Support microSD/microSDHC/microSDXC card,up to 512GB Support smart surveillance 
Support human/vehicle classification 
Operating conditions -30℃~65℃(-22℉~149℉), ≤95%RH


DC12V±10%, PoE:IEEE 802.3at 
IP66
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SPECIFICATIONS
	Camera 
	

	Image Sensor 
	1/2.8"CMOS 

	Min. Illumination 
	Color:0.001lux@ (F1.5,AGC ON),B/W:0lux with IR 

	Shutter Time 
	1s~1/100000s 

	Day&Night 
	IR-cut filter with auto switch (ICR) 

	Smart IR 
	Yes 

	WDR 
	120dB 

	S/N 
	42dB 

	Lens 
	

	Focal Length 
	5mm~115mm 

	Optical Zoom 
	23X 

	Zoom Speed 
	<5s 

	Aperture Range 
	F1.5~F3.0 

	Aperture Type 
	Auto(P-Iris) 

	Field of View 
	55.8°~3.2°(H); 32.2°~1.8°(V); 61°~3.64°(D) 

	Focus Control 
	Auto/Semi-auto/Manual 

	Close Focus Distance 
	1000mm~1500mm 

	DORI Distance 
	Detect:1351m 
Observe:536m 
Recognize:270m 
Identify:135m 

	Pan&Tilt 
	

	Pan Range 
	0~360°(P) 





	Pan Speed 
	Manual Speed:0.1°～80°/s 
Preset Speed:80°/s 

	Tilt Range 
	-16°~90°(T) (Default -3°~90°(T)) 

	Tilt Speed 
	Manual Speed:0.1°～80°/s 
Preset:80°/s 

	3D Position 
	Yes 

	Preset 
	500 

	Cruise 
	16(up to 32 presets per cruise) 

	Scan 
	8 

	Pattern 
	8,each with 600s memory or 1000 orders 

	Scheduled Task 
	Preset,Cruise,Scan,Pattern 

	North Point 
	Yes(Manual setting) 

	Power-off Memory 
	Yes 

	Illuminator 
	

	IR LEDs 
	7 

	IR Distance 
	Up to 150m 

	Wavelength 
	850nm 

	IR Irradiation Angle 
	Yes 

	Compression Standard 
	

	Video Compression 
	S+265/H.265/H.264B/H.264M/H.264H/Motion JPEG 

	Video Bit Rate 
	32Kbps~16Mbps 

	Audio Compression 
	G.711A/G.711U/ADPCM_D/AAC_LC 

	Audio Sampling Rate 
	8kHz/32kHz/48kHz 

	Image 
	

	Max. Resolution 
	2MP,1920×1080@30fps 

	Main Stream 
	PAL:25fps(1920×1080,1280×720,640×480,704×576) NTSC:30fps(1920×1080,1280×720,640×480,704×480) 

	Sub Stream 
	PAL:25fps(704×576,704×288,640×360,352×288) NTSC:30fps(704×480,704×240,640×360,352×240) 





	Third Stream 
	PAL:25fps(352×288) 
NTSC:30fps(352×240) 

	BLC 
	Yes 

	HLC 
	Yes 

	AGC 
	Yes 

	3DNR 
	Yes 

	White Balance 
	Auto/Semi-Auto/Manual/Sunshine/Nature Light/Warmlight Lamp/Daylight Lamp/ Filament Lamp/Lock White Balance 

	ROI 
	7 Dynamic Areas for Both Main and Sub Stream 

	OSD 
	5 regions(Each region can have a maximum of 127 characters ,up to 1 line); 16*16/24*24/32*32/48*48/64*64/adaptable size; Vector/Lattice 

	Defog 
	Yes 

	Flip 
	Normal/Horizontal Mirror/Vertical Mirror/Inverted Flip 

	Regional Exposure 
	Yes 

	Regional Focus 
	Yes 

	Demist 
	Yes 

	Feature 
	

	General Alarm 
	Motion Detection; Mask Alarm; Alarm Input 

	Exceptions Alarm 
	Voltage Alarm; Disk Full; Disk R/W Error; Recording Exception; IP Address Conflict; MAC Address Conflict; FTP Server Exception ; Network cable disconnected 

	Linkage Method 
	Send Email; Trigger Sound; Trigger Recording; Trigger Capture; Notify Surveillance Center; Alarm Output 

	Video Analytics 
	Human/Vehicle Classification; Tripwire; Double Tripwire; Perimeter; Object Abandon; Object Missing; Heatmap; Video Abnormal; Audio Abnormal 

	Network 
	

	ANR 
	Yes 

	Protocols 
	RTSP; RTMP; HTTP; HTTPS; TCP/IP; UDP; UPnP; ICMP; IGMP; SNMP v1\v2\v3; DHCP; DNS; DDNS; Easy DDNS; NTP; SMTP; TLS v1.2; SSL; 802.1x; QoS; IPv4; IPv6; PPPoE; SSH; Unicast; Multicast; ARP; RTP; SRTP; FTP; SFTP 

	System Compatibility 
	P2P; ONVIF(Profile S/T/G/M); SDK; CGI; Milestone; RTSP; RTMP; HTTP PUSH 

	Remote Connection 
	≤2 





	User/Host 
	32users, 
Level 4:Admin/Browse/Browse+Control/Browse+Control+Set 

	Client 
	Easy7 VMS 

	Mobile Client 
	EasyLive Plus 

	Web 
	IE10+; Firefox52+; Edge89+; Safari11+; Chrome57+ 

	Interface 
	

	Communication Interface 
	1*RJ45 (10/100Base-T) 

	Audio I/O 
	1*Input Impedance 1kΩ,2.0~2.4Vp-p; 1*Output Impedance 600Ω 

	Alarm I/O 
	1*Switching; 1*Switching,Voltage≤DC24V,Current≤1A 

	Reset Button 
	Yes 

	On-board Storage 
	Support microSD/microSDHC/microSDXC card,up to 512GB 

	General 
	

	Web Client Language 
	19 languages 
Simple Chinese/English/Traditional Chinese/Spanish/Italian/ Korean/Turkish/Russian/ Thai/ Polish/French/Dutch/ Hebraism/Vietnamese/Arabic/German/ Ukrainian / Portuguese/Albanian 

	Operating Temperature 
	-30℃~65℃(-22℉~149℉) 

	Operating Humidity 
	≤95%RH 

	Storage Temperature 
	-30℃~65℃(-22℉~149℉) 

	Storage Humidity 
	10%~95%RH(non-condensing) 

	Power Supply 
	DC12V±10%; PoE:IEEE 802.3at 

	Power Consumption 
	7.15W(IR OFF) ; 18.5W(IR ON) 

	Protection 
	Surge4000V; ESD6000V; IP66 

	Material 
	Metal+plastic 

	Boundary Dimensions 
	161(D)276(H)mm 

	Package Dimensions 
	260(L)260(W)465(H)mm 

	GrossWeight 
	3.8kg 

	NetWeight 
	2.1kg 





DIMENSIONS (Unit: mm) 
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Assembly diagram of Junction Box 
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