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TC-R3110 Spec:I/B/L/Eu/V1.1 1HDD 10ch NVR
SK Series
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KEY FEATURES 
Up to 10-ch IP camera accesses 
Incoming/Outgoing bandwidth: 60Mbps/40Mbps 
S+265, H.265, S+264, H.264, S+265 V2.0 video formats Max. decoding capability: 8MP(30fps)×1 or 1080P(30fps)×6 4-ch synchronous playback 
Up to 8 TB capacity for each HDD 
Simultaneous HDMI and VGA outputs 
HDMI output at up to 4K resolution
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1×RJ-45, 10/100 Mbps self-adaptive Ethernet port 
S+ 265 compression effectively reduces the storage space by up to 75% Support cloud upgrade
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SPECIFICATIONS
	Video and Audio 
	

	Access Channel 
	10 

	Incoming Bandwidth 
	60Mbps 

	Outgoing Bandwidth 
	40Mbps 

	Resolution 
	8MP/6MP/5MP/4MP/3MP/1080P/UXGA/720P/VGA/4CIF/DCIF/2CIF/CIF/QCIF 

	Preview Decoding Capability 
	8MP(30fps)×1, 6MP(30fps)×2, 5MP(30fps)×2, 4MP(30fps)×3, 3MP(30fps)×4, 1080P(30fps)×6, 720P(30fps)×10, 4CIF(30fps)×10 

	Playback Decoding Capability 
	8MP(30fps)×1, 6MP(30fps)×2, 5MP(30fps)×2, 4MP(30fps)×3, 3MP(30fps)×4, 1080P(30fps)×4, 720P(30fps)×4, 4CIF(30fps)×4 

	Third-party Camera Access 
	ONVIF(Profile S/T); RTSP 

	HDMI Output 
	HDMI: 1024×768(60Hz), (720P )1280×720(50Hz/60Hz), 1280×800(60Hz), 1366×768(60Hz), 1440×900(60Hz), (1080P)1920×1080(50Hz/60Hz), (4K)3840×2160(30Hz) 

	VGA Output 
	VGA: 1024×768(60Hz), (720P )1280×720(50Hz/60Hz), 1280×800(60Hz), 1366×768(60Hz), 1440×900(60Hz), (1080P)1920×1080(50Hz/60Hz) 

	Multi-screen Display 
	Simultaneous Output: 
VGA: 1/2A/2B/3/4/5/6/7/8/9/10 
HDMI: 1/2A/2B/3/4/5/6/7/8/9/10 

	Compression Standard 
	

	Video Compression 
	S+265; H.265; S+264; H.264; S+265 V2.0 

	Audio Compression 
	G.711A; G.711U; ADPCM_D 

	Stream Type 
	Video; Video & Audio 

	Network 
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	Network Protocol 
	802.1X; ARP; DDNS; DHCP; DNS; Easy DDNS; HTTP; HTTPS; ICMP; IGMP; IPv4; IPv6; Multicast; NTP; RTCP; RTP; RTSP; SMTP; SRTP; SSH; TLSv1.2; TCP; UDP; Unicast; UPnP 

	Client 
	Easy7 VMS (Win, MAC OS) 

	Mobile Client 
	EasyLive Plus (Android, iOS) 

	System Compatibility 
	RTSP; CGI; SDK; P2P 

	Web 
	IE10+; Firefox52+; Edge89+; Safari11+; Chrome57+ 

	Recording Playback 
	

	Multi-channel Playback 
	4 

	Record Mode 
	Manual Recording; Alarm Recording; Schedule Recording; Smart Storage Mode 

	Storage Method 
	Local HDD 

	Backup 
	USB storage device 

	Playback Function 
	Play/Pause/Stop/Slow/Speed/Backwards 30s/Forwards 30s/Full Screen/Backup (Video Editing)/ Step/Digital Zoom/Instant Replay 

	Dual Stream Record 
	Yes 

	Alarm 
	

	General Alarm 
	Motion Detection; Mask Alarm; Alarm Input(IPC) 

	Exceptions Alarm 
	Video Loss; Network Disconnected; No Disk; Illegal Access; Disk group space alert; Disk Full; Disk R/W Error; Recording Abnormal; Abnormal found in smart of disk; Abnormal temperature of the disk; Voltage Alarm(IPC); RTC Failure; IP Address Conflict; MAC Address Conflict; Disk Overload 

	Intelligent Analytics 
	

	AI by Camera 
	Tripwire; Double Tripwire; Perimeter; Object Abandon; Object Missing; Running; Parking; Loitering; Video Abnormal; Audio Abnormal; On Duty Detection; Crowd Detection; Smart Alarm; Human/ Vehicle Classification 

	Search 
	

	VCA Search 
	Early-warning Search; Behavior Search; Duty Search; Smart Motion Detection 

	Storage 
	

	HDD Capacity 
	Up to 8 TB capacity for each HDD 

	Disk Group 
	1 Disk Group 

	External Port 
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	USB 
	2×USB2.0 

	HDMI 
	1×HDMI(supports up to 4K resolution output) 

	VGA 
	1×VGA 

	Network Interface 
	1×RJ-45, 10/100 Mbps self-adaptive Ethernet port 

	SATA 
	1×SATA interface 

	General 
	

	UI Language 
	English; Spanish; Italian; Turkish; French; Polish; Hebrew; German; Portuguese; Greek 

	Power Supply 
	DC12V 

	Power Consumption 
	<10W(HDD not included, idling) 

	NetWeight 
	0.4 kg 

	GrossWeight 
	0.7 kg 

	Boundary Dimensions 
	201(L)202(W)43(H)mm 

	Package Dimensions 
	315(L)70(W)235(H)mm 

	Operating Temperature 
	-10℃~+55℃ (+14℉~+131℉) 

	Operating Humidity 
	10%~90%RH (non-condensing) 

	Storage Temperature 
	-20℃~+60℃ (-4℉~+140℉) 

	Package Kit 
	Network Video Recorder*1; Screw Pack*1; Mouse*1; European Standard Power Adapter(DC12V 1.5A)*1; Instructions*1; Parts List*1 
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DIMENSIONS (Unit: mm) 
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Physical Interfaces 
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