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TC-C35MS 4LHB-27135 
Dome Camera
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[image: ]
KEY FEATURES 
Metal housing 
Up to 5MP,2880×1620@30fps 
S+265/H.265/H.264B/H.264M/H.264H/Motion JPEG 
Color:0.002Lux@(F1.6,AGC ON),B/W:0Lux with IR 
IR range up to 50m 
1×Built-in Mic 
Support microSD/microSDHC/microSDXC card,up to 512GB Support smart surveillance, face capture
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Support human/vehicle/non-motor vehicle/pet(cat、dog) classification Operating conditions -35℃~65℃(-31℉~149℉), ≤95%RH 
DC12V±25%,Max. 8.5W, PoE:IEEE 802.3at,Max. 9.5W 
IP66, IK10
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SPECIFICATIONS
	Camera 
	

	Image Sensor 
	1/2.7"CMOS 

	Min. Illumination 
	Color:0.002Lux@(F1.6,AGC ON),B/W:0Lux with IR 

	Shutter Time 
	1s~1/100000s 

	Day&Night 
	IR-cut filter with auto switch (ICR) 

	Smart IR 
	Yes 

	WDR 
	120dB,True WDR(TWDR) 

	S/N 
	>42dB 

	Angle Adjustment 
	0~345°(P); 0~90°(T); 0~350°(R) 

	Lens 
	

	Lens Type 
	Motorized 

	Focal Length 
	2.7~13.5mm 

	Lens Mount 
	Φ14 

	Aperture Range 
	F1.6 

	Aperture Type 
	Fixed 

	Field of View 
	102°~33.2°(H); 56.7°~18.7°(V); 125.7°~38°(D) 

	DORI Distance 
	Detect:60m~220m 
Observe:24m~87m 
Recognize:12m~44m 
Identify:6m~22m 

	Illuminator 
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	IR LEDs 
	16 

	IR Distance 
	Up to 50m 

	Wavelength 
	850nm 

	White LEDs 
	8 

	Whitelight Distance 
	15m 

	Compression Standard 
	

	Video Compression 
	S+265/H.265/H.264B/H.264M/H.264H/Motion JPEG 

	Video Bit Rate 
	32k~16Mbps 

	Audio Compression 
	G.711A/G.711U/ADPCM_D/AAC_LC 

	Audio Sampling Rate 
	8kHz/32kHz/48kHz 

	Image 
	

	Max. Resolution 
	5MP,2880×1620@30fps 

	Main Stream 
	PAL:25fps(2880×1620,2688×1520, 2560×1440, 2304×1296)50fps(1920×1080, 1280×720) NTSC:30fps(2880×1620,2688×1520, 2560×1440, 2304×1296)60fps(1920×1080, 1280×720) 

	Sub Stream 
	PAL:25fps(704×576, 704×288, 640×360, 352×288) NTSC:30fps(704×480, 704×240, 640×360, 352×240) 

	Third Stream 
	PAL:25fps(1280x720,704x576,704x288,352x288, 640×480) NTSC:30fps(1280x720,704x480,704x240,352x240, 640×480) 

	BLC 
	Yes 

	HLC 
	Yes 

	AGC 
	Yes 

	3D DNR 
	Yes 

	White Balance 
	Auto/Semi-Auto/Manual/Sunshine/Nature Light/Warmlight Lamp/Daylight Lamp/Filament Lamp/ Lock White Balance 

	ROI 
	8 rectangular static areas 

	Corridor Mode 
	Yes 

	OSD 
	Overlay of additional characters in 5 regions,2 line, with a maximum of 127 characters or 42 Chinese characters per region; 16*16/24*24/32*32/48*48/64*64/96*96,Default Adaptive; Vector/ Lattice 


2026.03.20


[image: ]
	Picture Overlay 
	1*200x200 size BMP 24 color bit image overlay 

	Privacy Mask 
	4 black static areas 

	Defog 
	Yes 

	Feature 
	

	General Alarm 
	Motion Detection; Mask Alarm; Alarm Input 

	Exceptions Alarm 
	Voltage Alarm; Disk Full; Disk R/W Error; IP Address Conflict; MAC Address Conflict; FTP Server Exception ; Network Disconnection; No Disk; Illegal Access 

	Linkage Method 
	Send Email; Trigger Sound; Trigger Warmlight; Trigger Recording; Trigger Capture; Notify Surveillance Center; Alarm Output; Trigger smart light 

	Video Analytics 
	Human/Vehicle/Non-motor Vehicle/Pet(Cat、Dog) Classification; Tripwire; Perimeter; Video Abnormal; Audio Abnormal 

	Rules of Behavior Analyse In 1 Scene 
	8 

	Face Mode 
	Face Capture 

	Face Detection Performance 
	Detect up to 8 faces at the same scene; Capture up to4 faces at the same scene 

	False Rate of Face Capture 
	≤1% 

	Face Duplicate Capture Rate 
	≤20%（Continuous 4-person scene and below） 

	Mask Attribute Linkage Alarm 
	Mask Attribute Linkage Alarm 

	Image Push Strategy 
	Image Push Strategy 

	Image Push Interval 
	Image Push Interval 

	Capture Mode 
	Capture Mode 

	Face Capture 
	Face Capture 

	Background Image Resolution 
	1920*1080 

	Background Image OSD Overlay 
	video streamOSD/customize 

	Network 
	

	ANR 
	Yes 
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	Protocols 
	RTSP; RTMP; HTTP; HTTPS; TCP; UDP; UPnP; ICMP; IGMP; SNMP v1\v2\v3; DHCP; DNS; DDNS; Easy DDNS; NTP; SMTP; TLS v1.2; SSL; 802.1X; QoS; IPv4; IPv6; PPPoE; SSH; Unicast; Multicast; RTCP; ARP; SRTP; FTP; SFTP; NAS 

	System Compatibility 
	ONVIF(Profile S/T/G/M) ; SDK; CGI; Milestone 

	Remote Connection 
	Up to 7 channels 

	Client 
	Easy7 VMS 

	Mobile Client 
	EasyLive Plus 

	Web 
	IE10+; Firefox52+; Edge89+; Safari11+; Chrome57+ 

	Interface 
	

	Communication Interface 
	1×RJ-45 (10/100 Base-T) 

	Audio I/O 
	1×input, two-core , max. input amplitude:3.3 Vpp, input impedance:1 KΩ, interface type:non-equilibrium; 1×output, two-core, max. output amplitude:3.3 Vpp, output impedance:100 Ω, interface type: non-equilibrium 

	Alarm I/O 
	1×input,TTL,3mA,3.3VDC; 1×output,TTL,30mA,12VDC 

	Built-in Mic 
	1×Built-in Mic 

	Reset Button 
	Yes 

	On-board Storage 
	Support microSD/microSDHC/microSDXC card,up to 512GB 

	RTC 
	Yes 

	General 
	

	Web Client Language 
	20 languages 
Simple Chinese/Traditional Chinese/English/Spanish/Korean/Italian/Turkish/Russian/Thai/French/ Polish/Dutch/Hebrew/Arabic/Vietnamese/German/Ukrainian/Portuguese/Albanian/Greek 

	Operating Temperature 
	-35℃~65℃(-31℉~149℉) 

	Operating Humidity 
	≤95%RH 

	Storage Temperature 
	-40℃~65℃(-40℉~149℉) 

	Storage Humidity 
	10%~95%RH(non-condensing) 

	Power Supply 
	DC12V±25%,Max. 8.5W; PoE:IEEE 802.3at,Max. 9.5W 

	Protection 
	Surge4000V; ESD6000V; IP66; IK10 

	Boundary Dimensions 
	143(L)143(W)123(H)mm 
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	Package Dimensions 
	250(L)180(W)175(H)mm 

	GrossWeight 
	1.18kg 

	NetWeight 
	0.9kg 


DIMENSIONS (Unit: mm) 
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Assembly diagram of Junction Box 
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