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TC-C38MS 4LHB-27135 
Dome Camera
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KEY FEATURES 
Metal housing 
Up to 8MP,3840×2160@30fps 
S+265/H.265/H.264B/H.264M/H.264H/Motion JPEG 
Color:0.002Lux@(F1.6,AGC ON),B/W:0Lux with IR 
IR range up to 50m 
1×Built-in Mic 
Support microSD/microSDHC/microSDXC card,up to 512GB Support smart surveillance
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Support human/vehicle/non-motor vehicle/pet(cat、dog) classification Operating conditions -35℃~65℃(-31℉~149℉), ≤95%RH 
DC12V±25%,Max. 11W, PoE:IEEE 802.3at,Max. 12.5W 
IP66, IK10
[image: ]
SPECIFICATIONS
	Camera 
	

	Image Sensor 
	1/2.8"CMOS 

	Min. Illumination 
	Color:0.002Lux@(F1.6,AGC ON),B/W:0Lux with IR 

	Shutter Time 
	1s~1/100000s 

	Day&Night 
	IR-cut filter with auto switch (ICR) 

	Smart IR 
	Yes 

	WDR 
	120dB,True WDR(TWDR) 

	S/N 
	>42dB 

	Angle Adjustment 
	0~345°(P); 0~90°(T); 0~350°(R) 

	Lens 
	

	Lens Type 
	Motorized 

	Focal Length 
	2.7~13.5mm 

	Lens Mount 
	Φ14 

	Aperture Range 
	F1.6 

	Aperture Type 
	Fixed 

	Field of View 
	107°~32.3°(H); 54.6°~18.2°(V); 130°~35°(D) 

	DORI Distance 
	Detect:82m~331m 
Observe:32m~120m 
Recognize:16.5m~60.5m 
Identify:8m~30m 

	Illuminator 
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	IR LEDs 
	16 

	IR Distance 
	Up to 50m 

	Wavelength 
	850nm 

	White LEDs 
	8 

	Whitelight Distance 
	15m 

	Compression Standard 
	

	Video Compression 
	S+265/H.265/H.264B/H.264M/H.264H/Motion JPEG 

	Video Bit Rate 
	32k~16Mbps 

	Audio Compression 
	G.711A/G.711U/ADPCM_D/AAC_LC 

	Audio Sampling Rate 
	8kHz/32kHz/48kHz 

	Image 
	

	Max. Resolution 
	8MP,3840×2160@30fps 

	Main Stream 
	PAL:25fps(3840×2160, 3200×1800,2560×1440, 2304×1296)50fps(1920×1080, 1280×720) NTSC:30fps(3840×2160, 3200×1800,2560×1440, 2304×1296)60fps(1920×1080, 1280×720) 

	Sub Stream 
	PAL:25fps(704×576, 704×288, 640×360, 352×288) NTSC:30fps(704×480, 704×240, 640×360, 352×240) 

	Third Stream 
	PAL:25fps(704×576, 704×288, 352×288, 640×480) NTSC:30fps(704×480, 704×240, 352×240, 640×480) 

	BLC 
	Yes 

	HLC 
	Yes 

	AGC 
	Yes 

	3D DNR 
	Yes 

	White Balance 
	Auto/Semi-Auto/Manual/Sunshine/Nature Light/Warmlight Lamp/Daylight Lamp/Filament Lamp/ Lock White Balance 

	ROI 
	8 rectangular static areas 

	Corridor Mode 
	Yes 

	OSD 
	Overlay of additional characters in 5 regions,2 line, with a maximum of 127 characters or 42 Chinese characters per region; 16*16/24*24/32*32/48*48/64*64/96*96,Default Adaptive; Vector/ Lattice 
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	Picture Overlay 
	1*200x200 size BMP 24 color bit image overlay 

	Privacy Mask 
	4 black static areas 

	Defog 
	Yes 

	Feature 
	

	General Alarm 
	Motion Detection; Mask Alarm; Alarm Input 

	Exceptions Alarm 
	Voltage Alarm; Disk Full; Disk R/W Error; IP Address Conflict; MAC Address Conflict; FTP Server Exception ; Network Disconnection; No Disk; Illegal Access 

	Linkage Method 
	Send Email; Trigger Sound; Trigger Warmlight; Trigger Recording; Trigger Capture; Notify Surveillance Center; Alarm Output; Trigger smart light 

	Video Analytics 
	Human/Vehicle/Non-motor Vehicle/Pet(Cat、Dog) Classification; Tripwire; Double Tripwire; Perimeter; Object Abandon; Object Missing; Heatmap; Loitering; Running; Parking; People Counting; Crowed Detection; Safety Helmet Detection; On Duty Detection; Video Abnormal; Audio Abnormal 

	Rules of Behavior Analyse In 1 Scene 
	8 

	Network 
	

	ANR 
	Yes 

	Protocols 
	RTSP; RTMP; HTTP; HTTPS; TCP; UDP; UPnP; ICMP; IGMP; SNMP v1\v2\v3; DHCP; DNS; DDNS; Easy DDNS; NTP; SMTP; TLS v1.2; SSL; 802.1X; QoS; IPv4; IPv6; PPPoE; SSH; Unicast; Multicast; RTCP; ARP; SRTP; FTP; SFTP; NAS 

	System Compatibility 
	ONVIF(Profile S/T/G/M) ; SDK; CGI; Milestone 

	Remote Connection 
	Up to 7 channels 

	Client 
	Easy7 VMS 

	Mobile Client 
	EasyLive Plus 

	Web 
	IE10+; Firefox52+; Edge89+; Safari11+; Chrome57+ 

	Interface 
	

	Communication Interface 
	1×RJ-45 (10/100 Base-T) 

	Audio I/O 
	1×input, two-core , max. input amplitude:3.3 Vpp, input impedance:1 KΩ, interface type:non-equilibrium; 1×output, two-core, max. output amplitude:3.3 Vpp, output impedance:100 Ω, interface type: non-equilibrium 

	Alarm I/O 
	2×input,TTL,3mA,3.3VDC; 1×output,relay,1A,24VDC 
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	Built-in Mic 
	1×Built-in Mic 

	Reset Button 
	Yes 

	On-board Storage 
	Support microSD/microSDHC/microSDXC card,up to 512GB 

	RTC 
	Yes 

	Additional Interfaces 
	RS-485 

	General 
	

	Web Client Language 
	20 languages 
Simple Chinese/Traditional Chinese/English/Spanish/Korean/Italian/Turkish/Russian/Thai/French/ Polish/Dutch/Hebrew/Arabic/Vietnamese/German/Ukrainian/Portuguese/Albanian/Greek 

	Operating Temperature 
	-35℃~65℃(-31℉~149℉) 

	Operating Humidity 
	≤95%RH 

	Storage Temperature 
	-40℃~65℃(-40℉~149℉) 

	Storage Humidity 
	10%~95%RH(non-condensing) 

	Power Supply 
	DC12V±25%,Max. 11W; PoE:IEEE 802.3at,Max. 12.5W 

	Protection 
	Surge4000V; ESD6000V; IP66; IK10 

	Boundary Dimensions 
	143(L)143(W)123(H)mm 

	Package Dimensions 
	250(L)180(W)175(H)mm 

	GrossWeight 
	1.18kg 

	NetWeight 
	0.9kg 


2026.03.20


[image: ]
DIMENSIONS (Unit: mm) 
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Assembly diagram of Junction Box 
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